Partially Unreadable Sign

FUEL GAUGE CALIBRATED TO

THRUST LINE INCIDENCE, USE

CHART FOR OTHER INCIDENCES

CAUTION

LANDING GEAR EXTENSION LEVER

TO REMAIN IN “DOWN” POSITION

WHEN AIRPLANE IS ON THE GROUND

ACTUAL

CAPACITY

TANKS

1 & 2

360 U.S. GALS.

300 IMP GALS.

TANKS

3 & 4

121 U.S. GALS.

101 IMP. GALS.

TANKS

5 & ^

250 U.G. GALS.

208 IMP. GALS.

WARNING

DISCONNECT PLUG

WHEN TORPEDO IS

NOT INSTALLED